# Matching reference output style

Example solved cases live in `examples/`. Each includes:

## Global scalars (in `case_data.yml`)

- **Cl** — lift coefficient
- **Cd** — drag coefficient

## Volume/surface fields (in `case_data_0.vtu`)

| Field | Description |
|-------|-------------|
| Cp | Pressure coefficient |
| Ux, Uy | Velocity components |
| p | Pressure |
| nut | Turbulent kinematic viscosity |
| nuTilda | SA turbulence working variable |

`case_meta.yml` lists fields and `num_points` (expect ~21 812 points on the reference mesh).

## For ML / submit pipeline

- Train on mesh + fields; predict the same field names at holdout AoA.
- For leaderboard submit, export **Cl_pred**, **Cd_pred** per case in the Rescale evaluation JSON layout
  (see `submit/README.md`).
